Hole:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Defect Number** | : | 0184 | | |
| **Defect Name** | : | Hole | | |
| **Defect Type** | : | Isolated Defects | | |
| **Fabric Type** | : | Double Knit Fabrics | | |
| **Description** | | | | |
| Hole — This is the result of a lint ball interfering with the normal interloping of the yarn.  Severity: Major  Category: III | | | | |
| **Defect Number** | | | : | 0183 | |
| **Defect Name** | | | : | Hole | |
| **Defect Type** | | | : | Finishing Defects | |
| **Fabric Type** | | | : | Single Knit Fabrics | |
| **Description** | | | | | |
| Hole — This is where the fabric has been pulverized during compaction. This is the back of the fabric.  Severity: Major  Category: V | | | | | |