Run:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Defect Number** | | | : | 0174 | |
| **Defect Name** | | | : | Run | |
| **Defect Type** | | | : | Warp lines, vertical lines | |
| **Fabric Type** | | | : | Single Knit Fabrics | |
| **Description** | | | | | |
| Run — This a vertical line of unformed stitches resulting from a broken needle or jack.  Severity: Major  Category: I | | | | | |
| **Defect Number** | : | 0179 | | |
| **Defect Name** | : | Needle Line | | |
| **Defect Type** | : | Warp lines, vertical lines | | |
| **Fabric Type** | : | Double Knit Fabrics | | |
| **Description** | | | | |
| Needle Line — The result of a bent needle.  Severity: Minor  Category: I | | | | |